**Be-Line® wall-mounted toilet brush set with lid**

Model with anti-theft lock for fixing

Metallised anthracite 304 stainless steel

Reference: **4051C**

Specification description

Wall-mounted toilet brush set with lid from the Be-Line® range.

Robust toilet brush set with anti-theft lock for fixing.

Bacteriostatic metallised anthracite powder-coated 304 stainless steel.

Easy to clean: plastic bowl can be removed from above.

Plastic bowl with reservoir: prevents the brush from sitting in stagnant water and splashing when next used.

Toilet brush and lid automatically centre in the holder.

Stainless steel thickness: 1mm body.

Dimensions: Ø 90 x 410mm.

30-year warranty.