**Twin hole pre-rinse set with mixer**

With bib tap

Black flexible hose L. 95cm and ergonomic controls

Reference: **5633UK**

Specification description

Complete pre-rinse set with bib tap adapted to intensive use in professional kitchens.

Deck-mounted twin hole mixer with 180mm centres with:

- Valve heads with reinforced mechanisms with ergonomic control levers.

- Offset inlet connections with M1/2" tails.

Bib tap with swivelling, tubular spout L. 200mm:

- 25 lpm full flow rate achieved within the first 90°.

- Valve head with reinforced mechanism with ergonomic control lever.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref. 433010).

Hand spray with anti-scale nozzle and shock-resistant tip.

Black, reinforced, food-grade flexible hose L. 0.95m.

3/4" stainless steel column.

Adjustable wall bracket.

Stainless steel spring guide.

Pre-rinse set with 30-year warranty.

These pre-rinse models can be installed close to the splashback.