**Twin hole pre-rinse set with mixer**

Without bib tap

Black flexible hose L. 95cm and ergonomic controls

Reference: **5680UK**

Specification description

Complete pre-rinse set without bib tap, adapted for intensive use in professional kitchens.

Rim-mounted twin hole mixer with 180mm centres with:

- Valve heads with reinforced mechanisms with ergonomic control levers.

- Offset inlet connections with M1/2" tails.

Black hand spray with adjustable jet and 9 lpm flow rate at the outlet (ref: 433010).

Hand spray with antiscale nozzle and shock-resistant tip.

Black, reinforced, food-grade flexible hose L. 0.95m.

3/4" stainless steel column.

Adjustable wall bracket.

Stainless steel spring guide.

Twin hole pre-rinse set with 30-year warranty.

These pre-rinse models can be installed close to the splashback.