**SECURITHERM EP pressure-balancing sink mixer**

Single hole, single control tall mixer with EP cartridge

Removable swivelling stainless steel spout H.320mm

Reference: **2870T3EP**

Specification description

Deck-mounted SECURITHERM pressure-balancing high sink mixer.

Single hole, single control mixer with high, swivelling spout H. 320mm.

Mixer supplied with 2 removable stainless steel spouts.

Total anti-scalding safety: reduced HW flow if CW supply fails (and vice versa).

Constant temperature regardless of variations in pressure and flow rate.

Ø 35mm ceramic cartridge with pressure-balancing and pre-set maximum temperature limiter.

Body and spout with smooth interiors (limits bacterial development).

Thermal shocks are possible without removing the control lever or shutting off the cold water supply.

Flow rate limited to 9 lpm at 3 bar.

Body and base in chrome plated brass.

Hygiene control lever L. 185mm requires no manual contact.

PEX flexibles F3/8" with filters and non-return valves.

Reinforced fixing via 2 stainless steel rods.

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics

Suitable for people with reduced mobility.

30-year warranty.