**Mechanical basin mixer**

Single hole, single control tall mixer with ceramic cartridge

Mechanical mixer with fixed spout H.205 L.170

Reference: **2565T5**

Specification description

Deck-mounted mechanical basin mixer.

Single hole, single control mixer with fixed spout H. 205mm L. 170mm.

Tall mixer with BIOSAFE hygienic outlet suitable for fitting a BIOFIL point-of-use filter.

Ø 35 classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (limits bacterial development).

Thermal shocks are possible without removing the control lever or shutting off the cold water supply.

Flow rate regulated at 5 lpm.

Chrome-plated brass body and base.

Hygiene control lever L. 185mm requires no manual contact.

PEX flexibles F3/8".

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.