**SPORTING 2 SECURITHERM electronic shower panel**

Battery-operated, thermostatic, rain-effect spray, kit 2/2

Concealed inlet, anodised aluminium

Reference: **714916**

Specification description

SPORTING 2 SECURITHERM, thermostatic electronic shower panel, kit 2/2:

Recessed inlets.

Anodised aluminium and chrome-plated satin finish panel.

Slimline structure with concealed fixings

Battery-operated with CR123 6V Lithium batteries.

Infrared presence detection. Shower starts when hand is moved towards the sensor (detection distance ~4cm).

Shuts off voluntarily or automatically after ~60 seconds.

Duty flush (~60 seconds every 24 hours after the last use).

Flow rate 6 lpm at 3 bar.

Tamperproof, rain-effect fixed shower head with automatic flow rate regulation.

Accessible filters and non-return valves.

Integrated stopcocks.

M½" connections (Compact nanny joint, kit 1/2).

Electronic shower panel suitable for people with reduced mobility.

30-year warranty.

SECURITHERM technology:

Thermostatic mixer directly integrated in the head of the shower panel.

Temperature set by the installer.

Stable temperature, pre-set at 38°C.

Anti-scalding failsafe: automatic shut-off if the cold water fails.

Anti-cold showers function: automatic shut-off if the hot water fails.

Order with support bracket 714612.