**SECURITHERM shower panel**

Thermostatic time flow

Top inlet, handset, aluminium

Reference: **792370**

Specification description

Thermostatic time flow shower panel:

Anodised aluminium shower panel for wall-mounted, exposed installation.

Top inlet via in-line stopcocks M½".

SECURITHERM thermostatic mixer.

Adjustable temperature control from cold water up to 38°C; with 1st limiter set at 38°C and 2nd limiter set at 41°C.

Anti-scalding failsafe: automatic shut-off if the cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Thermal shocks are possible.

Soft-touch operation.

Handset with removable flexible via rapid push-fit STOP connector.

~30-second time flow valve for control of sliding handset on chrome-plated rail.

Flow rate 6 lpm at 3 bar.

Concealed fixings.

Filters and non-return valves.

Suitable for people with reduced mobility.

30-year warranty.