**Mechanical basin mixer**

Single hole mechanical mixer H. 95mm L.120mm

Solid control lever

Reference: **2721T**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mixer with a curved spout H. 95mm L. 120mm fitted with a hygienic BIOSAFE outlet.

Spout suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduced bacterial development).

Flow rate limited to 5 lpm.

Solid control lever.

Without pop-up waste.

F3/8" PEX flexibles.

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with copper tails.