**Mechanical mixer for sinks or troughs**

Single control single hole tall mixer with ceramic cartridge

Mechanical mixer with swivelling spout H.165 L.140

Reference: **2564T1**

Specification description

Deck-mounted mechanical basin mixer.

Single control single hole mixer with swivelling spout H. 165mm L. 140mm.

Tall mixer with BIOSAFE hygienic outlet suitable for fitting a BIOFIL point-of-use filter.

Ø 35mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduces bacterial development).

Thermal shocks are easy to undertake without removing the control lever or shutting off the cold water.

Flow rate regulated at 5 lpm.

Chrome-plated body, base and spout.

Hygiene control lever L. 185mm requires no manual contact.

PEX flexibles F3/8".

Fixings reinforced by 2 stainless steel rods and back-nuts.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.