**Single hole pre-rinse set with mixer**

With bib tap and swivelling tubular spout

Black flexible with scale-resistant hand spray

Reference: **5825**

Specification description

Complete pre-rinse set with bib tap.

Deck-mounted, single hole mixer with slimline control lever.

Suitable for intensive use in professional kitchens.

Supplied with F3/8" flexible connectors and non-return valves.

Bib tap with swivelling tubular spout L. 200mm.

- full flow rate 16 lpm within a 90° turn.

- valve head with reinforced mechanism and ergonomic control.

Black hand spray with adjustable jet and 10 lpm flow rate at the outlet (ref. 433009).

Scale-resistant hand spray with shock-resistant tip.

Black, reinforced, food-grade flexible hose L. 0.95m.

¾" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.