**Deck-mounted single-hole mixer - 60 lpm**

Swivelling spout H. 685mm L. 300mm

With extension column

Reference: **5652**

Specification description

Deck-mounted single hole mixer with extension column for installation on stove tops.

Swivelling tubular spout Ø 22mm, H. 685mm L. 300mm with hygienic flow straightener.

Ceramic cartridge Ø 45mm.

Flow rate 60 lpm at 3 bar.

Spout with smooth interior.

Slimline control lever.

Chrome-plated brass body and spout.

Soldered copper pipe water inlets.

Reinforced fixing.

30-year warranty.