**Single hole pre-rinse mixer set**

Without bib tap

Black flexible and scale-resistant handset

Reference: **5830**

Specification description

Complete pre-rinse set with no bib tap, suitable for intensive use in professional kitchens.

Deck-mounted single hole mixer with:

- valve heads with reinforced mechanisms and ergonomic controls.

- F3/8" flexible connectors and non-return valves.

- fixings reinforced by 2 threaded rods and back-nuts.

Black handset with adjustable jet with 10 lpm flow rate at the outlet (ref. 433009).

Scale-resistant handset with shock-resistant tip.

Black, reinforced food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.