**TEK washbasin with 2 buttons**

Polished satin 304 stainless steel - Wall-mounted w/ concealed outlet

With integrated tap

Reference: **161360**

Specification description

Wall-mounted hand washbasin.

Bacteriostatic 304 stainless steel.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Vandal-resistant: shrouded basin, concealed trap.

Supplied with a time flow valve: stainless steel tamperproof push-button and anti-blocking system, time flow 7 seconds.

With 2 buttons cold water/mixed water.

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Without overflow.

Supplied with trap.

Supplied with fixing elements.

CE marked. Complies with European standard EN 14688.

Weight: 8.6kg.