**BLACK BINOPTIC electronic tap**

Mains supply, L. 200mm

Recessed, smooth interior spout

Reference: **379ENCB**

Specification description

Recessed electronic basin tap:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Filter and solenoid valve M3/8".

Chrome-plated brass body.

Matte black chrome finish.

Recessed installation.

Anti-blocking safety.

Spout with smooth interior and low volume of water (limits bacterial niches).

Suitable for people with reduced mobility.

30-year warranty.