**BLACK BINOPTIC MIX electronic mixer**

Mains supply, L. 230mm

CW 110 mm, standard lever, smooth interior spout

Reference: **379MCHB**

Specification description

Cross wall matte black electronic basin mixer:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Filters and solenoid valves M3/8".

Chrome-plated brass body.

Matte black chrome finish.

Cross wall installation ≤110mm

Cable for sensor, flexibles and mounting all pass through the same hole.

Anti-blocking safety.

Spout with smooth interior and low volume of water (reduces bacterial niches).

Side temperature control with standard lever and adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.