**TEMPOSTOP time flow tap 2 controls**

Anti-blocking version (AB)

Cross wall TC, M½"

Reference: **748210**

Specification description

Time flow basin tap for cross wall installation:

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

2 controls: 1 button for mixed water and 1 button for cold water.

Tamperproof scale-resistant flow straightener.

Chrome-plated solid brass body M½".

Control ≤ 200mm, spout ≤ 230mm.

Ligature-resistant button is flush to wall.

Anti-rotating pin and back nut.

AB anti-blocking system: water will flow only when the push-button is released.

30-year warranty.