**TEMPOMATIC 4 electronic tap**

Integrated batteries

Wall-mounted L. 130mm, Integr electronics, Refit

Reference: **443436**

Specification description

Wall-mounted electronic basin tap:

Battery-operated with integrated 123 6V Lithium batteries.

Reduced-stagnation solenoid valve and electronic unit integrated into the body of the tap.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Active infrared presence detection, sensor at the end of the spout optimises detection.

Chrome-plated stainless steel body L. 130mm.

Cap fixed in place by 2 concealed screws.

Anti-blocking security.

Stopcock.

Wall-mounted.

Suitable for people with reduced mobility.

30-year warranty.