**TEMPOCHASSE direct flush valve**

Direct flush WC valve

Cross wall 200mm

Reference: **760110**

Specification description

Flush system without cistern: directly connected to pipework.

For walls ≤ 200mm.

Time flow ~7 seconds.

Vacuum breaker.

Inline stopcock and flow rate/volume adjuster.

Chrome-plated metal body.

Shock-resistant mechanism.

Inline inlet F1".

Connection washer Ø 32/55mm.

Threaded rod can be cut to size.

Base flow rate: 1 l/sec at 1 bar dynamic pressure.

Compatible with rain water.

30-year warranty.

[Formerly ref: 760150]