**TEMPOCHASSE direct flush kit**

Direct flush WC valve

Cross wall 200mm with PVC tube

Reference: **760210**

Specification description

Flush system without cistern: directly connected to pipework.

For walls ≤ 200mm.

Time flow ~7 seconds.

Vacuum breaker.

In-line solid brass stopcock and flush volume/flow rate adjuster.

Chrome-plated metal body.

Shock-resistant mechanism.

In-line supply F1".

Connection washer Ø 32mm/55mm.

Cut-to-size threaded rod.

With PVC elbow flush tube Ø 32 mm.

Base flow rate: 1 l/sec at 1 bar dynamic pressure.

Compatible with rain water.

30-year warranty.

[Formerly ref: 760700]