**Mechanical mixer for sinks or troughs**

High swivelling spout H. 300mm L. 250mm

Mechanical mixer with swivelling spout H.305 L.220

Reference: **2564T4**

Specification description

Deck-mounted mechanical sink mixer.

Single hole, single control mixer with swivelling spout H. 305mm L. 220mm.

Tall mixer with hygienic flow straightener suitable for fitting a BIOFIL terminal filter.

Ø 35mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduced bacterial development).

Thermal shocks are easy to undertake without removing the control lever or shutting off the cold water supply.

Flow rate limited to 9 lpm at 3 bar.

Chrome-plated brass body and spout.

Hygiene control lever L. 185mm requires no manual contact.

PEX flexibles F3/8".

Fixings reinforced by 2 stainless steel rods and back-nuts.

Mechanical mixer ideal for people with healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.