**SECURITHERM thermostatic sequential sink mixer**

Single hole thermostatic sequential mixer H. 160mm L. 140mm

Hygiene lever L. 146mm, copper tails

Reference: **H9620610**

Specification description

Deck-mounted SECURITHERM thermostatic sink mixer.

Thermostatic sequential mixer: opens and closes with cold water.

Single hole mixer with curved spout H. 160mm L. 140mm with hygienic flow straightener for no impurity retention and thermal shock-resistant.

Anti-scalding failsafe: automatic shut-off if cold or hot water supply fails.

Securitouch thermal insulation prevents burns.

No risk of cross flow between hot and cold water.

No non-return valves on the inlets.

Scale-resistant sequential thermostatic cartridge for single lever control of flow rate and temperature.

Temperature can be adjusted from cold water up to 40°C with temperature limiter set at 40°C.

Tested without water to comply with NHS requirements. No pre-set temperature.

Thermal or chemical shocks are possible.

Body and spout with smooth interiors and low water volume.

Flow rate regulated at 9 lpm.

No manual contact thanks to Hygiene control lever L. 146mm.

No pop-up waste.

Supplied with copper tails with chrome-plated brass stopcocks.

Reinforced fixing via 2 stainless steel rods.

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Suitable for people with reduced mobility.

30-year warranty.

Also available with PEX flexibles.