**SECURITHERM thermostatic shower mixer**

Thermostatic mixer without non-return valves

With inline STOP/CHECK wall connectors

Reference: **H9768TP**

Specification description

SECURITHERM dual control thermostatic shower mixer.

Thermostatic mixer with no non-return valves on the inlets (reduced bacterial proliferation).

No risk of cross flow between hot and cold water.

Mixer with anti-scalding failsafe: shuts off automatically if cold water supply fails.

Prevents cold showers: shuts off automatically if hot water supply fails.

Securitouch thermal insulation prevents burns.

Scale-resistant thermostatic cartridge for temperature adjustment.

¼-turn ceramic head for flow rate adjustment.

Temperature control up to 43°C.

Maximum temperature limiter pre-set to 38°C.

Thermal shocks are possible without shutting off the cold water.

Flow rate limited to 9 lpm at 3 bar.

ERGO controls.

M½" shower outlet.

F¾" inlets with integrated filters.

Mixer with inline STOP/CHECK wall connectors M1/2" M3/4".

Mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Mixer suitable for people with reduced mobility.

Shower mixer with 30-year warranty.