**BIOSAFE mechanical basin mixer**

Single hole mechanical mixer H. 100mm L. 110mm

Hygiene control lever L. 150mm

Reference: **2920L**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mixer with spout H. 100mm L. 110mm fitted with a BIOSAFE hygienic outlet.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Spout with a tube with a smooth interior, no niches where bacteria can develop, and low water volume.

The speed with which the water flows through the tube considerably reduces biofilm development.

Thermal shocks are possible without removing the lever or shutting off the cold water supply.

Body with very flow water volume (reduces bacterial development).

Flow rate regulated at 5 lpm.

Hygiene control lever L. 150mm.

Ergonomic, brass pop-up waste 1 1/4".

F3/8" PEX flexibles.

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.