**TEMPOMIX 3 shower mixer**

Time flow control, kit 2/2

Recessed, chrome-plated metal control

Reference: **794218**

Specification description

Recessed time flow shower with soft-touch operation kit 2/2:

Tamperproof chrome-plated metal control plate 160 x 160mm.

Operation and temperature selection on control button.

Maximum temperature limiter (can be adjusted by installer).

Time flow ~30 seconds, can be adjusted.

Soft-touch operation.

Flow rate 6 lpm at 3 bar.

Suitable for people with reduced mobility.

30-year warranty.

Order with recessed waterproof housing ref. 794BOX1.