**Recessed waterproof housing for TEMPOMIX shower**

Recessed, kit 1/2

Waterproof

Reference: **790BOX**

Specification description

Recessed waterproof housing kit 1/2.

For TEMPOMIX shower mixer.

Partition thickness can be between 10 to 30mm.

30-year warranty.

Order with control plate references 790218 or 790219.