**TEMPOMIX time flow shower mixer**

Time flow single control, kit 2/2

Waterproof recessed, chrome-plated metal control

Reference: **790218**

Specification description

Recessed time flow shower mixer kit 2/2:

Tamperproof bright polished stainless steel control plate 160 x 220mm.

TEMPOMIX ¾" single control shower mixer.

Ligature-resistant collar.

Temperature control and operation via the control.

Maximum temperature limiter (can be adjusted by the installer).

Time flow ~30 seconds, soft-touch operation.

Flow rate 12 lpm at 3 bar, can be adjusted.

Concealed fixings, stopcocks M½".

Chrome-plated metal control.

Integrated non-return valves and filters.

30-year warranty.

Order with recessed waterproof housing ref. 790BOX.