**TEMPOSTOP time flow shower valve**

Time flow, kit 2/2

Recessed waterproof housing, Bayblend® control

Reference: **749218**

Specification description

Recessed time flow shower kit 2/2:

Tamperproof polished stainless steel control plate 160 x 220mm.

TEMPOSTOP ¾" time flow valve for mixed water supply.

Ligature-resistant ring.

Time flow ~30 seconds.

Flow rate 12 lpm at 3 bar, can be adjusted.

Solid brass body.

Concealed fixings.

M½" stopcock with filter.

Chrome-plated Bayblend® control.

30-year warranty.

Order with waterproof housing ref. 749BOX.