**BINOPTIC wall-mounted electronic soap dispenser**

Liquid or foam soap dispenser

Mains, black 304 stainless steel, cross wall

Reference: **512111BK**

Specification description

Wall-mounted electronic soap dispenser.

Liquid or foam soap dispenser.

Vandal-resistant model for cross wall installation for walls up to 110mm.

No manual contact: infrared cell detects hands automatically.

Matte black 304 stainless steel spout.

No waste pump dispenser.

Separate electronic unit and removable tank for installation beneath the washbasin or in a service duct.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with maximum viscosity of 3,000 mPa.s or specific foam soap.

Total spout length: 115mm.

Supplied with flexible tube 1.20m for remote tanks.

30-year warranty.

CE marked.