**TEMPOMATIC 4 deck-mounted electronic soap dispenser**

TEMPOMATIC 4 electronic soap dispenser

Mains, chromed 304 stainless steel, 0.5L tank

Reference: **512531P**

Specification description

Deck-mounted electronic soap dispenser.

Liquid soap, foam soap or hydroalcoholic gel dispenser.

No manual contact: hands are automatically detected by infrared cell.

Chrome-plated 304 stainless steel spout.

No-waste pump dispenser.

Removable, separate electronic unit and tank for installation beneath the counter top.

Automatic soap dispenser: mains supply with 230/6V transformer.

For vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or special foam soap.

Compatible with hydroalcoholic gel.

Spout length: 111 mm.

Supplied with 0.5 litre tank.

30-year warranty.

CE marked.