**FINO design-led urinal**

Matte black 304 stainless steel - rear inlet

Reference: **135710BK**

Specification description

Wall-hung individual rimless urinal.

Compatible with all standard frame systems on the market.

Bacteriostatic 304 stainless steel. Stainless steel thickness: 1.2mm.

Matte black Teflon® finish.

Rear water inlet (recessed).

Recessed or exposed horizontal waste outlet.

Concealed trap.

Quick and easy to install to from the front thanks to a stainless steel mounting frame.

Supplied with a 1½" P trap. Supplied with fixing elements.

CE marked. Complies with European standard EN 13407 for a 2-litre flush.

Weight: 3.5kg.

30-year warranty.