**S21 P floor-standing WC pan**

Matte black 304 stainless steel

Reference: **110300BK**

Specification description

Floor-standing WC pan.

Elegant and simple design.

Bacteriostatic 304 stainless steel. Stainless steel thickness: 1.5mm.

Matte black Teflon® finish..

One-piece pressed WC bowl, seam-free for easy maintenance and better hygiene

Concealed perimetral flushing rim.

Horizontal water inlet: Ø 55mm.

Horizontal waste outlet: Ø 100mm. Supplied with PVC pipe.

Water saving: works with 4L or more of water.

Pre-drilled holes for fixing the toilet seat. Supplied with stainless steel blanking caps when installed without toilet seat lid.

Quick and easy to install: 2 access panels with theft prevention TORX security screws.

CE marked. Complies with European standard EN 997 for 4L flush.

Weight: 14kg.

30-year warranty.