**Vandal-resistant push-fit BIOFIL connector M24/125**

For wall-mounted showers or shower panels

Reference: **821125**

Specification description

Push-fit connector M24/125 for wall-mounted fixed showers or shower panels.

For quick and easy installation of filtration devices on wall-mounted showers or a DELABIE shower panel (SPORTING, SECURITHERM, etc.).

Vandal-resistant model: tamperproof connector to avoid any vandalism or unauthorised use or removal of the filter.

30-year warranty.