**Recessed housing for thermostatic shower mixers**

Sequential mixer, kit 1/2

Recessed, waterproof

Reference: **H96BOX**

Specification description

Recessed waterproof housing for thermostatic sequential shower mixers, kit 1/2:

- Collar with waterproof seal.

- Hydraulic connection to the outside and maintenance from the front.

- Water supply connects to the top.

- Adjusts to all types of installation (rails, solid walls, panels).

- Compatible with wall finishes from 10 - 120mm (while maintaining the minimum recessing depth of 80mm).

- Suitable for standard or "pipe-in-pipe" supply.

- Stopcocks and flow rate adjustment, filters and cartridge are all integrated and accessible from the front.

- Thermostatic sequential shower mixer.

- Supplied in 2 kits: secure system flush without sensitive elements.

30-year warranty.

Order with control-plate reference H9631.