**Detector**

For BINOPTIC and TEMPOMATIC 2

With 1.5m cable

Reference: **CEL378150V**

Specification description

Detector.

For BINOPTIC and TEMPOMATIC 2 basin controls.

With 1.5m cable.