**Time flow cartridge**

For TEMPOMIX basin mixers

Time flow ~7 seconds

Reference: **743791**

Specification description

Time flow cartridge for TEMPOMIX basin mixers.

For TEMPOMIX basin mixers type 795000 and 795100 new design.

Time flow ~7 seconds.

Flow rate can be adjusted from 1.4 - 6 lpm.