**Time flow cartridge**

For TEMPOMIX basin mixers

Time flow ~7 seconds

Reference: **743798**

Specification description

Time flow cartridge for TEMPOMIX basin mixers.

For cross wall TEMPOMIX basin mixers type 795209 old design.

Time flow ~7 seconds.

Flow rate can be adjusted from 1.4 - 6 lpm.