**Be-Line® matte black angled grab bar 135°, 400 x 400mm**

Matte black aluminium, 3 fixing points

Ø 35mm with ergonomic flat face

Reference: **511982BK**

Specification description

Be-line® angled grab bar 135°, Ø 35mm, for people with reduced mobility.

For use as a handrail (horizontal part) or as a grab rail (135° part), for WCs, showers or baths.

Use as a universal grab bar for either left or right side.

Aluminium tube thickness 3mm. Solid aluminium fixing points.

Rounded profile Ø 35mm with ergonomic flat front face that prevents rotation for an optimal grip.

Matte black powder-coated finish; provides a good visual contrast with light-coloured walls.

Uniform surface for easy maintenance and hygiene.

38mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

3 fixing points prevent the hand from getting trapped and simplify installation.

Concealed fixings.

Supplied with stainless steel screws Ø 8 x 70mm for concrete walls.

Dimensions: 400 x 400mm.

Tested to over 200kg. Maximum recommended user weight: 135kg.

Grab bars for toilets with 30-year warranty. CE marked.