**BINOPTIC MIX 2 electronic basin mixer**

Mains, recessed, stopcocks, L. 240mm

Smooth interior spout, satin, standard lever

Reference: **484000**

Specification description

Recessed satin electronic basin mixer:

230/6V mains supply.

Reduced-stagnation solenoid valve and electronic unit are integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 - 6 lpm.

Scale-resistant aerator.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Wall-mounted stainless steel mixer.

Active, infrared presence detection, sensor at the end of the spout optimises detection.

Anti-blocking security.

Spout with smooth interior and low water volume (reduces bacterial development).

Side temperature control with adjustable maximum temperature limiter on mixers.

Set duty flush and launch thermal shocks manually.

Suitable for people with reduced mobility.

30-year warranty.