**Thermostatic sequential cartridge**

SECURITHERM thermostatic cartridge

For the H961x range

Reference: **N961**

Specification description

Thermostatic cartridge for wall-mounted sequential mixers.

SECURITHERM cartridge for H9610/H9611 range.