**TEMPOMIX 3 time flow basin mixer**

Soft-touch operation, deck-mounted, H.250

Single control

Reference: **794120**

Specification description

Deck-mounted single control time flow basin mixer:

Soft-touch operation.

Temperature control and operation on the push-button.

Time flow pre-set at ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 3 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Chrome-plated stainless steel body, 250mm height for deck-mounting.

F3/8" PEX flexibles with filters and non-return valves.

Fixing reinforced by back-nut.

Adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.