**Be-Line® DOC M matte black straight grab bar, 600mm**

Matte black powder-coated aluminium

Ø 35mm

Reference: **511906MBK**

Specification description

Be-Line® DOC M grab bar Ø 35mm, for people with reduced mobility.

For use as a handrail or grab bar for WCs, showers or baths.

Aluminium tube, 3mm thick. Solid aluminium fixing points.

Rounded profile Ø 35mm with ergonomic flat front face that prevents rotation for an optimal grip.

Matte black powder-coated finish provides a good visual contrast with the wall.

Uniform surface for easy maintenance and hygiene.

60mm gap between the bar and the wall: minimal space prevents the forearm passing between the bar and the wall, reducing the risk of fracture in case of loss of balance.

Concealed fixings.

Supplied with stainless steel screws Ø 8 x 70mm for concrete walls.

600mm centre-to-centre.

Tested to over 200kg. Maximum recommended user weight: 135kg.

30-year warranty. CE marked.

Complies with DOC M.