**Time flow cartridge**

For TEMPOSTOP and TEMPOMIX 2 cross wall/lever

Time flow ~15 seconds, AB anti-blocking system

Reference: **743215**

Specification description

Time flow cartridge for TEMPOSTOP and TEMPOMIX 2 cross wall/lever.

Time flow ~15 seconds.

AB anti-blocking system.