**SPORTING 2 SECURITHERM time flow shower panel**

Thermostatic, scale-resistant nozzle

Concealed inlet, anodised aluminium

Reference: **714735**

Specification description

Thermostatic time flow shower panel:

Anodised aluminium and chrome-plated satin finish panel.

Slimline structure with concealed fixings.

Soft-touch operation.

Automatic mechanical flush with each use.

Time flow ~30 seconds.

Flow rate 6 lpm at 3 bar.

Tamperproof, scale-resistant fixed shower head with automatic flow rate regulation.

Accessible filters and non-return valves.

Integrated stopcocks.

M½" connection.

Suitable for people with reduced mobility.

30-year warranty.

SECURITHERM technology:

Thermostatic shower mixer directly integrated in the head of the shower panel.

Temperature set by the installer.

Stable temperature, pre-set at 38°C.

Anti-scalding failsafe: automatic shut-off if the cold water fails.

Anti-cold showers function: automatic shut-off if the hot water fails.