**BLACK BINOPTIC electronic tap**

Mains supply

TC 190mm, spout with smooth interior, L. 205mm

Reference: **379DERB**

Specification description

Matte black cross wall electronic basin tap:

Independent IP65 electronic control unit.

230/12V mains supply with transformer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Adjustable duty flush (pre-set flush ~60 seconds every 24 hours after last use).

Active, infrared movement detection, sensor at the end of the spout optimises detection.

Filter, solenoid valve M3/8".

Chrome-plated solid brass body.

Matte black chrome finish.

Chrome-plated spout L. 205mm for cross wall installation ≤ 190mm.

Sensor cable L.120mm, flexibles and mounting all pass through the same hole.

Anti-blocking security.

Spout with a smooth interior and low water volume (limits bacterial niches).

Suitable for people with reduced mobility.

30-year warranty.