**TEMPOSTOP 3 time flow urinal flush valve**

Time flow 3 seconds

Angled 1/2"

Reference: **703800**

Specification description

Exposed time flow urinal flush valve.

For stalls, standard or siphon action urinals.

For wall-mounted installation.

Time flow ~3 seconds.

Flow rate pre-set at 0.15 l/sec. at 3 bar, can be adjusted.

Compatible with rain water.

Chrome-plated solid brass body M½".

Wall plate.

Angled for recessed installation.

30-year warranty.