**Wall-mounted CANAL wash trough**

Polished satin 304 stainless steel - L. 2400mm

With 4 Ø 22mm tap holes

Reference: **121300**

Specification description

Wall-mounted wash trough, for 4 services - 2,400mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 0.8mm for the bowl, 1.5mm for surround and fixing brackets.

Easy to install: no joint concealers to install, lightweight trough.

Water controls can be installed wall-mounted or deck-mounted.

Drainage on the right.

With x4 Ø 22mm tap holes.

Supplied with M1"1/4 hygienic concave grid waste. Without overflow.

Supplied with fixings.

CE marked. Complies with European standard EN 14296.

Weight: 13kg.

Possible to add a bacteriostatic 304 stainless steel splashback (ref. 100300).

30-year warranty.