**Nanny joint for recessed water inlets**

Mains supply, Kit 1/2

Reference: **484012**

Specification description

Nanny joint for recessed water inlet, Kit 1/2 :

For wall-mounted TEMPOMATIC MIX 4, connects directly to the pipework.

Compatible with mains supply 230/6V.

Adaptable installation (plaster rails, solid walls, panels).

Compatible with wall finishes from 0 to 35mm.

Secured system purge without sensitive elements.

30-year warranty.

Order with basin mixer references 493500 or 493400.