**Sequential mechanical basin mixer**

Sequential mechanical mixer with fixed spout L. 200mm

With standard offset connectors

Reference: **2437S**

Specification description

Wall-mounted sequential mechanical basin mixer.

Sequential mechanical mixer: opens and closes with cold water within a 90° turning range.

Wall-mounted mixer with flat, fixed under spout L. 200mm with hygienic flow straightener.

Securitouch thermal insulation prevents burns.

Ø 35mm classic ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume.

The water velocity in the tubes reduces biofilm development considerably.

Flow rate regulated at 5 lpm.

Chrome-plated brass body.

Hygiene control lever L. 200mm requires no manual contact.

Mixer supplied with offset standard wall connectors.

Recommended installation height: 110 - 200mm above the top of the basin.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Sequential mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.