**Nanny joint for recessed water inlets**

Inlet only without mixer

Kit 1/2

Reference: **794012**

Specification description

Nanny joint for recessed inlet, Kit 1/2 :

For TEMPOFLUX 3 wall-mounted, connection directly to pipework.

Modulable installation (plaster rails, solid walls, panel).

Compatible with wall finishes from 10 to 30mm.

Secure system flush without sensitive elements.

30-year warranty.