

TEMPOMATIC 7 deck-mounted electronic basin tap - tall model



Reference: F7EV1002


Specification description

Deck-mounted electronic basin tap.

230/6.75V mains supply or battery-operated with CR-P2 6V Lithium batteries (To be ordered separately).

Infrared presence sensor in the tap body.

Integrated 5.7 lpm flow rate regulator.

Adjustable, vandal-resistant aerator.

Adjustable duty flush (~ 30 seconds every 24 hours since last use).

316 stainless steel body, satin finish.

F3/8" PEX flexibles with filter.

Fixing reinforced by back-nut.

Anti-blocking security.

Drop height: 245mm.

Suitable for people with reduced mobility.

30-year warranty.
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